

**Experiment-15**

**Configuration of DHCP (dynamic host configuration protocol) in packet Tracer.**

**Step1:** 1 Server, 1Switch and 4 PCs



**Step2:** connect fast ethernets from Switch to PCs



**Step3:** Assign IP address for each PCs


IP address for PC0:192.168.0.1

IP address for PC1: 192.168.0.2

IP address for PC2: 192.168.0.3

IP address for PC3: 192.168.0.4

**Step4:** allocate the message



**Result:** message sent successfully from PC4-PC3